University of Macau

Faculty of Science and Technology



Debbis, The Deep Electrocardiogram Based Biometric Identification System

by

AxelAxel MS Mukwena, Student No: DB727501Dxxxxxx

Graduation Project Report submitted in partial fulfilment  
of the requirements of the Degree of   
Bachelor of Science in Computer Science

Project Supervisor

Prof. Liming ZHANG

05 June 2021

# 

DECLARATION

I sincerely declare that:

1. I and my teammates are the sole authors of this report,
2. All the information contained in this report is certain and correct to the best of my knowledge,
3. I declare that the thesis here submitted is original except for the source materials explicitly acknowledged and that this thesis or parts of this thesis have not been previously submitted for the same degree or for a different degree, and
4. I also acknowledge that I am aware of the Rules on Handling Student Academic Dishonesty and the Regulations of the Student Discipline of the University of Macau.

Signature : Shape

Description automatically generated with medium confidence

Name : Axel MS Mukwena

Student No. : DB727501

Date : 05 June 2021

ACKNOWLEDGEMENTS

The author would like to express his utmost gratitude to UM for providing the opportunity to carry out a project as a partial fulfilment of the requirement for the degree of Bachelor of Science.

I wish to express my sincere gratitude to several individuals and organizations for the utmost support and the opportunity to carry out a project as partial fulfilment for the Bachelor of Science degree. First, I wish to express my sincere gratitude to my supervisor, Professor Liming Zhang. Throughout the first semester of 2020/2021, her enthusiasm, patience, insightful comments, helpful information, practical advice, and unceasing ideas have helped me tremendously in my research and partial implementation of this project. Without her support and guidance, this project would not have been possible. I could not have imagined having a better supervisor in my study.

I also wish to express my sincere thanks to the University of Macau for providing me accessibility to numerous facilities and resources and the platform to apply and demonstrate what I have learned. Besides, I am deeply indebted to the Macau Foundation for granting me the scholarship while I continue to pursue my studies. This financial support continues to enable me to endure my studies at UM confidently.

Also, I am grateful to the several university Machine Learning Ph.D. scholars who provided me with guidance and directions in the past semester.

Finally, last but by no means least; also, to everyone in the Department of Computer and Information Science, it always great sharing premises with all of you, and I hope to continue doing so.

Thanks for all your encouragement!

**ABSTRACT**

With the rapid growth in authentication, there is an increased demand for individual identification and advanced security. While traditional methods for human identification such as passwords and tokens are easily accessible and implemented, they are prone to theft or loss. The Electrocardiogram (ECG) displays the potential to be used as a physiological signature for biometric systems because of its uniqueness, specificity, and unidimensional nature.

In this literature, I propose Debbis, the Deep Electrocardiogram Based Biometric Identification System. Through this, I demonstrate a novel Siamese neural architecture incorporating the Euclidean distance for biometric verification and deep convolutional neural networks based on multiresolution analysis for closed-set classification, both on time-series signal segments. I evaluated these methods using recordings from two major public databases: MIT-BIH and ECG-ID. Additional data were also recorded from active participants and simultaneously tested using an ECG monitoring device. Debbis achieved a competitive test accuracy score of 99.81% and validation loss of 0.82%. Furthermore, I simulated a biometric system using a web framework for model deployment and access testing and obtained state-of-the-art results with just 5-7 heartbeats as test samples.

.

TABLE OF CONTENTS

CHAPTER 1. INTRODUCTION 8

1.1 Biometric System 8

1.2 ECG as Biometric 8

1.3 Objectives, Motivation and Challenges 9

1.4 System Development, Environment and Resources 9

CHAPTER 2. LITERATURE SURVEY 11

CHAPTER 3. PROJECT EXECUTION SCHEDULE 13

CHAPTER 4. DESIGN 14

4.1 Goals 14

4.1.1 Enrolment 15

4.1.2 Verification 15

4.1.3 Authentication 16

4.2 Datasets 17

4.2.1 MIT-BIH 17

4.2.2 ECG-ID 17

4.3 Neural Network Architectures 17

CHAPTER 5. IMPLEMENTATION 18

5.1 Signal Acquisition 18

5.2 Signal Pre-processing 19

5.2.1 Peak Segmentation 20

5.2.2 Data Augmentation 20

5.3 Training Data 21

5.3.1 SNN Data 21

5.3.2 CNN Data 23

5.4 Network Architectures 25

5.4.1 Siamese Neural Network Structure 25

5.4.2 Convolutional Neural Network Architecture 26

CHAPTER 6. TESTING AND EVALUATION 27

6.1 Verification 27

6.2 Authentication. 28

CHAPTER 7. DISCUSSION 30

CHAPTER 8. ETHICS and PROFESSIONAL CONDUCT 31

CHAPTER 9. CONCLUSIONS 32

CHAPTER 10. REFERENCES 33

LIST OF FIGURES

[Figure 1: Segment representation of the Electrocardiogram. 9](#_Toc73211469)

[Figure 2: Gantt Chart of the work ditribution against time. 13](#_Toc73211470)

[Figure 3 First stage of the Biometric System. 14](#_Toc73211471)

[Figure 4 Second stage of the Biometric System 14](#_Toc73211472)

[Figure 5: Representation of the QRS complex 15](#_Toc73211473)

[Figure 6 Proposed approach of the Verification task 16](#_Toc73211474)

[Figure 7 Proposed approach of the Authentication task. 16](#_Toc73211475)

[Figure 8 a) Shows the BMD device used to extract signals; b) Demonstrate live signal Acquisition 18](#_Toc73211476)

[Figure 9 BMD Windows-OS Graphical User Interface 18](#_Toc73211477)

[Figure 10 Main contending ECG Segmentation Algorithm 20](#_Toc73211478)

[Figure 11 Illustrates the various augmentation methods 21](#_Toc73211479)

[Figure 12 Total training and test data distribution for SNN data 22](#_Toc73211480)

[Figure 13 Positive and Negative Pairs 23](#_Toc73211481)

[Figure 14 Total training and test data distribution for CNN data 23](#_Toc73211482)

[Figure 15 Illustrates the Siamese Neural Network Architecture 25](#_Toc73211483)

[Figure 16 Illustrates the Convolution Neural Network Architecture 26](#_Toc73211484)

[Figure 17 Training and Validation loss for the SNN model 27](#_Toc73211485)

[Figure 18 Training results for the SNN. In Blue is the Training loss and Red is Validation Loss 27](#_Toc73211486)

[Figure 19 Training and Validation Accuracy scores 28](#_Toc73211487)

[Figure 20 Training and Validation Loss scores 28](#_Toc73211488)

[Figure 21 Confusion Matrix of the CNN model 29](#_Toc73211489)

# INTRODUCTION

Since every existing authentication technique can be virtually compromised, institutions should not solely rely on any single control to grant access and authenticate individuals. With the advancement of technology and rising security concerns, more and more trustworthy authentication technologies are in demand [1].

## Biometric System

Biometrics are inherent physiological or behavioural characteristics typically used to identify and authenticate an individual digitally and grant them access to systems, devices, or information [2]. Any physiological or behavioural attribute can qualify as a biometric if it satisfies the criterion of being universal, distinctive, permanence, and collectible. Typically, a biometric system requires three modes of operation [3]:

* Enrolment: The biometric system collects the physiological or behavioural characteristics, process them through feature extraction, and store the extracted features as a template.
* Verification mode: The system verifies if the individual is enrolled by comparing the captured biometric features with the all the corresponding stored templates.
* Authentication: After a positive verification, the individual is classified against all enrolled individuals to assess if the verified individual is who they say they are.

While fingerprints and recently, iris and facial recognition are the most widely used biometrics, they are primarily prone to errors due to falsification [4]. This paves the way for the novel authentication approach, the Electrocardiogram (ECG) based biometric system.

## ECG as Biometric

ECG is a representation of the myocardial bioelectrical signal activity, reflected by periodic contractions and relaxation. These contractions and relaxation are caused by a change in voltage across the cell membrane of heart cells, creating a recordable continuous signal pattern [5]. Using external electrodes to record the signal, the ECG is represented by segments, each corresponding to a distinct stage of the cardiac cycle as illustrated in Figure 1. This morphological representation is unique to everyone [6], and it's such specificity among other attributes that make the ECG an appropriate biometric candidate.




Figure 1: Segment representation of the Electrocardiogram.

## Objectives, Motivation and Challenges

Because of its intrinsic and physiological origin, the ECG signal provides guaranteed uniqueness and permanence resulting in higher inter-individual variability [7]. Besides, it allows robustness against credentials falsification. Due to its general possession and presence in all users, ECG also provides a high degree of universality. ECG also verifies Liveness Detection by guaranteeing the biometric pattern is genuine in presenting individuals based on their inherent liveness property [7], unlike iris or fingerprints which require additional processing to establish the liveness of the reading. Therefore, the recognition systems based on ECG have higher security and reliability.

Despite its robustness, one of the main challenges of using ECG is the risk of abnormalities caused by morphological changes in the heart. Abnormal myocardial changes lead to a higher heart rate variability, reducing the system's recognition rate [8].

## System Development, Environment and Resources

As per the three modes of operations mentioned in [1.1 Biometric System](#_Biometric_System), the basic framework of the system begins with the extraction and storage of ECG feature-based templates into a memory-based model. The model is then deployed onto a Web API with an access point for biometric simulation where the user is validated and authenticated upon live ECG sample submitted.

The proposed system is experimented implemented with Python 3 Programming Language and additional Machine Learning toolkits and libraries [9]. Data pre-processing tasks were carried out on a Macintosh 2.4 GHz Quad-Core Intel Core i7 16 GB RAM computer. Sourced from the MIT-BIH and ECG-ID public databases, I carried out the data pre-processing tasks on a Macintosh 2.4 GHz Quad-Core Intel Core i7 16 GB RAM computer. Additional signal recordings of active participants were added and simultaneously tested using an ECG monitoring device. The ECG monitoring device is designed based on a BMD101 sensor chip and contains two dry metal electrodes acting as finger recording access points. I set up and trained both the Convolutional and Siamese Neural architecture model through the reproducible Google Colabolatory Notebook running on a Tesla P100-PCIE-16GB GPU.

Generally, the proposed task was executed over a period of a year course at the University of Macau, where 10% of the time was allocated to project and concept familiarity, 60% on data engineering and the rest of 30% on model development and deployment.

This work presents Debbis, an ECG-based biometric approach based on deep learning. I propose to use the novel Siamese neural architecture incorporating the Euclidean distance for biometric verification and template matching, and deep Convolutional Neural Networks (CNN) based on multiresolution analysis to extract features that allow performing a closed-set authentication. Furthermore, deploy the system onto a web platform enabling real-time simulation. The remaining of the report is organized in the following works: literature survey and related works, project execution, software design and implementation, testing and evaluation, discussion, ethics, and professional conduct and finally, conclusions.

# LITERATURE SURVEY

The ECG-based biometric system's design depends on the variability of several aspects, such as the number of leads analyzed, the type of features exploited, and the type of classifier used [10]. These aspects have a significant influence on the system's performance. Even though higher accuracy is associated with using multiple leads, one-lead ECG configuration is more widely accepted and suitable for biometrics because of its simplicity and speed during the signal acquisition phase [11].

In previous recognition research work [10] [12], the ECG-based biometric methods are divided into fiducial, non-fiducial classes. Fiducial methods use points of interest within the heartbeat wave P, Q, R, S and T illustrated in Figure 1, present in all healthy ECG signals. Non-fiducial techniques target extracting unique information from the ECG waveform without having to localize fiducial points. Some methods combine both fudicial and non-fiducial to form the partially fiducial approach which uses the R peak as a reference for waveforms segmentation, creating segments of QRS complex [12].

ECG recognition methodologies can also be classified based on the type of classifier used: k close neighbours, nearest middle, LDA, neural networks (NNs), generative model classifiers (GMCs), vector machines (SVMs) help, and others. Of these classes, nearest neighbour, nearest centre, and LDA are the most commonly used in ECG recognition literature [10]. A common concept is shared by all classifier-based systems whereby they analyze the ECG signal to extract meaningful features and use them as classifier inputs. For the same level of accuracy, Deep learning methods are more computationally and parametrically efficient. Deep learning methods can create deep data representations and learn new and more abstract representation of the input.

However, more recent work using Deep learning techniques such as Generic and Temporal Convolutional Neural Network (TCNN), Recurrent Neural Network (RNN) and Autoencoders for ECG-biometrics is emerging [13] [14] [15] [16]. Most of the work in the literature obtained promising results. However, they only considered closed-set biometric identification. Most studies did not explicitly illustrate that deep networks trained on samples obtained from a set of classes can be effectively used to confidently reject unknown classes. During realistic circumstances, unknown classes or imposters can emerge unexpectedly, which drastically weakens the robustness of these existing methods [17].

A classification task, rather than a recognition task, is being used in several studies [13] [14] [15] [16] [18]. In classification, we assume that there is a predefined set of classes from which we must discriminate. In terms of recognition, we assume that there are some classes that we can recognize within a much larger space of things we cannot recognize [19]. Verification problems for security-oriented ECG signals limit the target of interest to a single claimed identity while considering the set of all other possible people as potential impostors. There is a finite set of known individuals in a pool of unknown individuals, and labelling something new, novel or unknown should always be a valid outcome. This leads to what is sometimes called "open set" recognition [19].

Few deep learning methodologies have yet ventured into open-set recognition for ECG biometrics applications. There is noteworthy research into open-set recognition which uses one-shot learning [20] [21] [22] [23] [24]. One-shot learning heavily relies on knowledge transfer, using large datasets or learned features from state-of-the-art general-object detection or classification pre-trained models such as VGG19 [25] and Inceptionv3 (GoogLeNet) [26] for classification using few samples. Recent successful works in biometrics using 1D Electroencephalography (EEG) signals [27] [28], the use of the multimodal Siamese Neural Network (mSNN) have been employed. The novel mSNN model achieved a 98.57% classification accuracy outperforming the current state-of-the-art by 12.86% (in absolute terms)

On the other hand, Debbis attempts to combine Siamese Neural Network (SNN) based on Contrastive Loss for verification and CNNs for closed-set multi-class periodic re-authentication. The use of SNN and CNN individually have demonstrated superior accuracy in this context, thus employing them as combined steps towards accurate ECG individual identification will be vital.

# PROJECT EXECUTION SCHEDULE

Timeline

Description automatically generated

Figure 2: Gantt Chart of the work ditribution against time.

The Gantt chart in Figure 2 illustrates the work distribution against the project’s allocated period.

# DESIGN

The development of Debbis consists of two main stages:

* During development, signal acquisition and training of identity verification and authentication models was performed, Figure 3.
* The second stage includes the deployment of the trained models onto a simulated ECG signal secured web framework, Figure 4.

Diagram

Description automatically generated

Figure 3 First stage of the Biometric System.

Diagram

Description automatically generated

Figure 4 Second stage of the Biometric System

## Goals

In addition to the objectives in Chapter 1, the goals of Debbis also include allowing an efficient and accurate enrolment, verification, and authentication process. Hence, to achieve these goals, the biometric system should be robust, reliable, and unauthorizedly impenetrable.

### Enrolment

This process includes signal acquisition, feature extraction and feature preparation to train the verification and authentication models. One challenging task is identifying an optimal length of signals acquired which should guarantee the following requirements:

* Non-intrusive signal acquisition methods.
* The lowest possible amount of time during signal acquisition.
* Maximum signal length and minimal training time such that trustworthy predictive accuracy scores of the verifying and authenticating models are guaranteed.

A picture containing text, hanger

Description automatically generated

Figure 5: Representation of the QRS complex

During feature extraction, the main point of interest is the QRS complex,Figure 5, due to its central positioning, visual prominence and resistance to change during stress or emotional states [15]

### Verification

One major drawback of classification is the limitation to handle Unknown Unknown Classes (UUCs), i.e., classes with unseen features during training. Traditional recognition/classification algorithms have already achieved significant success in a variety of machine learning tasks when training and testing data are drawn from the same label and feature spaces [17].

Diagram

Description automatically generated

Figure 6 Proposed approach of the Verification task

A more realistic scenario, on the other hand, is usually open and non-stationary recognition/classification, such as in security systems, all non-enrolled individuals should be rejected with high confidence. To meet this challenge, Debbis achieves verification through open-set recognition whereby a Siamese neural network, Figure 6, matches the test signal to all the templates of the enrolled individuals, based on the Euclidean distance, and output the state of enrollment of the test individual on the system. Debbis no longer needs a “catch-all” class when it should reject a non-enrolled individual.

### Authentication

After a successful match, the test signal is authenticated through a closed-set multi-classification CNN, Figure 7. For the closed environment among a fixed set of persons: , the task is to develop a model that can identify person when given the persons’ ECG signal, .

Diagram

Description automatically generated

Figure 7 Proposed approach of the Authentication task.

## Datasets

To assess the performance in realistic conditions with a relevant number of users and an optimal record time with continuity, the MIT-BIH [29] and the ECG-ID [30] [31] public datasets from PhysioNet were chosen.

### MIT-BIH

Although the MIT-BIH Arrhythmia dataset [29] is focused on arrhythmia detection, it has also been used to benchmark biometric authentication accuracy in several works. This dataset contains ECG signals from 47 people who have arrhythmias of various types. The recordings were digitized at a sampling rate of 360 Hz with an 11-bit resolution over a signal range of 10 mV. Although the ECG signals were recorded in two channels, only the first channel was used in the proposed study.

### ECG-ID

The ECG-ID database [30] [31] is one of the few databases specifically created to investigate ECG-based authentication. As a result, this dataset has become the de facto choice for researchers working with ECG biometrics [Pinto]. In this dataset, 90 people had their ECG signals from lead I recorded for 20 seconds. Over a nominal 10 mV range, the signals were digitized at 500 Hz with a 12-bit resolution. 2 to 20 session data were collected for each subject. Thus, it is common practice among researchers to consider only two sessions for each person to avoid data imbalance [32] [33].

### BMD101 Sensor Chip

NeuroSky's BMD101 sensor chip is built with advanced analogue front-end circuitry and a flexible, strong digital signal processing structure. The development board has a Notch Filter and a Low Pass Filter. Typically, the Notch Filter is configured to be a 50Hz, 60Hz, or both notch through arrangement. For both 60Hz and 50Hz, the notch rejection is typically -63dB. The Low Pass Filter has a cut-off frequency of 100Hz. It has a consistent passband to the cut-off frequency and a -40dB passband at the stop frequency.

A picture containing text, electronics, computer

Description automatically generated

Figure 8 a) Shows the BMD device used to extract signals; b) Demonstrate live signal Acquisition

The device is non-intrusive and only requires the subject to hold the two dry metal electrodes with each of their thumbs, demonstrated in Figure 8.b and the signals are recorded and displayed through the GUI as illustrated in Figure 9. Signals were recorded from two individuals for durations of 20 min each. The device is very susceptible to noise hence it requires a low-noise place with minimal surface vibrations.

Diagram, schematic

Description automatically generated

Figure 9 BMD Windows-OS Graphical User Interface

## Neural Network Architectures

Creating a deep learning model for a single heartbeat-based authentication system is challenging because of limited signal duration and the need for large datasets. Short signals provide very little information for sequential input data which translates to the loss of considerable information. Thus, Debbis employed an extensive architecture capable of extracting complex features from each ECG segment. Both the Siamese and Convolutional Neural Networks employed a block structure inherited from VGG19 [25], amended to the needs of ECG features. Both structures contain a learning architecture with 30 layers, whereby between the input and the flatten layer, there exist 5 blocks. Each block contains a 1D Convolution, Batch Normalization, Activation and Max Pooling layer. The block structure allows connecting all the layers with matching feature-map sizes by stacking feature maps formed in earlier layers to feature maps at higher levels. More details on the neural network architectures are discussed in section 5.4.

# IMPLEMENTATION

## Signal Acquisition

Both the MIT-BIH and ECG-ID data files are stored in the Waveform Database (WFDB) file format. The record\_name.dat file formats are binary files containing samples of digitized signals. These files host waveforms, but they cannot be interpreted properly without their corresponding header files. The corresponding record\_name.hea files are short text files that describe the contents of associated signal files. I used the WFDB software package [34] to read and extract the signals and save them in an easily accessible and universally readable file format, record\_name.csv.

signals, = wfdb.rdsamp(file, sampfrom=0,

pn\_dir = os.path.join(database, folder))

df = pd.DataFrame(signals)

df.to\_csv(os.path.join(dir, folder, file + '.' 'csv'), index=False)

The BMD comes with a Windows-OS-compatible Graphical User Interface, Figure 9, to aid in the extraction of signals. A recording individual should be in place to begin, monitor and terminate the signal recording. The optimum signal duration was determined to be 20 minutes. The BMD GUI saves the signals in a datetime.txt file format as Figure.

# How the *datetime.txt* file looks like

timestamp: ADC HeartRate4sAverage HeartRate30sAverage

1621355037.727: 2696 95 92

1621355037.727: 1979 95 92

1621355037.727: 1093 95 92

1621355037.727: 812 95 92

1621355037.727: 1304 95 92

1621355037.727: 2055 95 92

1621355037.727: 2492 95 92

1621355037.727: 2575 95 92

1621355037.727: 2607 95 92

1621355037.727: 2682 95 92

1621355037.727: 2608 95 92

1621355037.727: 2241 95 92

1621355037.774: 1845 95 92

1621355037.774: 1744 95 92

1621355037.774: 1902 95 92

1621355037.774: 2008 95 92

1621355037.774: 2017 95 92

1621355037.774: 2174 95 92

1621355037.774: 2628 95 92

1621355037.774: 2978 95 92

1621355037.774: 2650 95 92

# Processing the *datetime.txt* file

with open('user\_id\_date.txt', 'r') as f:

for line in f:

value = int(line.strip().split()[1])

array.append(value)

# Normalize array to (-1, +1)

array = np.interp(array, (array.min(), array.max()), (-1, +1))

# Save to csv

df.to\_csv('user\_id\_date.csv', index=False)

## Signal Pre-processing

During this stage, the ECG signals are enhanced, and the most discriminating QRS complexes are extracted. No noise filtering was applied because different signal acquisition methods produced different noise levels and I couldn't access enough individuals to create a model trained purely from the data acquired using the BMD.

### Peak Segmentation

Chart, histogram

Description automatically generated

Figure 10 Main contending ECG Segmentation Algorithm

In the second step, I applied the christov and hamilton QRS segmentation algorithm presented in the literature [35] [36]. A comparison of the two algorithms is presented in figure 5. Among others, the christov algorithm demonstrates higher robustness, QRS and beat detection performance [37]. The algorithm filters the ECG through a sequence of moving averages, and a combination of adaptive thresholds is used for QRS detection. For the absence of any power-line interference, the first moving average filter is used. It is implemented as a Finite Impulse Response filter, where the number of coefficients in a 50 Hz duration is equal to the number of samples (20 ms). Similarly, with 28 ms, the second moving average is applied to decrease signal noise. The absolute value of the differential is then taken to illustrate the QRS complexes.

def segment(self, array):

peaks = ecg.christov\_segmenter(signal=array, sampling\_rate=500)[0]

for i in (peaks[1:-1]):

diff1 = abs(peaks[count - 1] - i)

diff2 = abs(peaks[count + 1] – i)

x = peaks[count - 1] + diff1 // 2

y = peaks[count + 1] - diff2 // 2

peakWave = array[x:y]

### Data Augmentation

Data augmentation is a technique used to create new training data from the existing one. Typical to popular geometrical augmentation methods typically applied to input data for CNN, such methods are not appropriate for this study. Signal waves have the characteristics of noise, pitch domain and time domain. The signal alterations will revolve around these characteristics in such a way that they only differ by a minimal factor from the original sample.

#### Noise Addition

This process involves the addition of Gaussian noise to the sample because of its normal distribution. Gaussian noises are random samples distributed at regular intervals with a mean of 0 and a standard deviation of 1.

factorValue = 0.09  
noiseAdding = array + factorValue \* np.random.normal(0, 1, len(array))

#### Pitch shifting

This process involves shifting the signal in the amplitude domain around the x−axis while minimally influencing the time domain.

factor = -0.3  
pitchShifting = librosa.effects.pitch\_shift(array, 500, n\_steps=float(factor))

#### Time Shifting

This process involves shifting the signal in the time domain around the y-axis while minimally influencing the x-axis.

samplingRate = 500  
timeShifting = np.roll(array, int(samplingRate / 150))

Chart, line chart, histogram

Description automatically generated

Figure 11 Illustrates the various augmentation methods

The variation outcome of these processes is demonstrated in Figure 11. After a successful pre-processing and augmentation, every individual's signal was saved to a pickle file format. After an assessment, only the MIT-BIH data and two individuals from the BMD were used because the ECG-ID did not have enough data to produce confident results.

## Training Data

### SNN Data

The ECG segments were cut to 700 per individual, hence a normal distribution of classes, Figure 12. The pre-processed data is normalized to values between 0-1. Data normalization helps get rid of several anomalies that can complicate the analysis of signals. Afterwards, the data is shuffled and placed into pairs. Each segment pair is either the same (1), meaning they belong to the same class or different (0), meaning they belong to different classes Figure 13. The data is then divided into training, validation and test sets to train and evaluate the performance of the classifier. The Sklearn selection model was used to randomly partition and allocate 60% of the data to training, 30% for validation and 10% for testing. The training set is used for classifier design, while the test set for performance and accuracy assessment.

Chart, background pattern

Description automatically generated

Figure 12 Total training and test data distribution for SNN data

# Normalize

x = (x - x.min()) / (x.max() - x.min())

y = np.array(y)

# Shuffle

# Create pairs

p = people

def create\_pairs(x, y):

yy, xx = [], []

indices = [np.where(y == i)[0] for i in p]

dic = {p[j]: indices[j] for j in range(len(p))}

for i in range(len(x)):

current\_image = x[i]

label = y[i]

ia = np.random.choice(dic[label], replace=False)

positive\_image = x[ia]

xx.append([current\_image, positive\_image])

yy.append(1)

choices = np.where(y != label)[0]

ib = np.random.choice(choices, replace=False)

negative\_image = x[ib]

xx.append([current\_image, negative\_image])

yy.append(0)

xx = np.array(xx)

yy = np.array(yy)

return xx, yy

x, y = create\_pairs(x, y)

Chart, line chart, histogram

Description automatically generated

Figure 13 Positive and Negative Pairs

### CNN Data

The ECG segments were cut to 10000 per individual, hence a normal distribution of classes, Figure 14. The pre-processed data is normalized to values between 0-1. Data normalization helps get rid of several anomalies that can complicate the analysis of signals. Afterwards, the data is shuffled and divided into training and validation sets to evaluate the performance of the classifier. The Sklearn selection model was used to randomly partition and allocate 60% of the data to training, 30% for validation and 10% for testing. The training set is used for classifier design, while the test set for performance and accuracy assessment.

Chart

Description automatically generated

Figure 14 Total training and test data distribution for CNN data

# Normalize

x = (x - x.min()) / (x.max() - x.min())

y = np.array(y)

# Shuffle for both SNN and CNN

# Train, Valid and test split

from sklearn.preprocessing import LabelBinarizer

# Determine segment shape (256)

SIG\_DIMS = (x.shape[1], 1)

# binarize the labels

lb = LabelBinarizer()

y = lb.fit\_transform(y)

# Split

x\_train, x\_test, y\_train, y\_test = train\_test\_split(

x, y, test\_size=0.4, shuffle=True, random\_state=42)

x\_valid, x\_test, y\_valid, y\_test = train\_test\_split(

x\_test, y\_test, test\_size=0.3, shuffle=True, random\_state=42)

x\_train = x\_train.reshape(x\_train.shape[0], SIG\_DIMS[0], SIG\_DIMS[1])

x\_valid = x\_valid.reshape(x\_valid.shape[0], SIG\_DIMS[0], SIG\_DIMS[1])

x\_test = x\_test.reshape(x\_test.shape[0], SIG\_DIMS[0], SIG\_DIMS[1])

## Network Architectures

### Siamese Neural Network Structure

The Siamese network contains two input fields for comparing two signal inputs and one output with a state value that corresponds to the similarity of the two signal segments [38]. To extract the features, two different sub-networks based on the structure inherited from the VGG19 [25] block architecture act on each input segment. The distance value is obtained by taking the cosine of the angle between two feature vectors. Figure 15 gives an overview of the proposed framework by applying Siamese network based on contrastive loss to determine if a person is enrolled or not.

### Convolutional Neural Network Architecture

Diagram

Description automatically generated

Figure 15 Illustrates the Siamese Neural Network Architecture

Diagram

Description automatically generated

Figure 16 Illustrates the Convolution Neural Network Architecture

# TESTING AND EVALUATION

In this experiment, both the SNN and CNN models are fed with 1D time-based ECG signals, each of length 256. Both networks had a Batch Size of 64, and learning rate of 0.00001, and used the Adam optimizer with decay. After numerous experiments, only the data from 39 candidates from MIT-BIH plus 1 candidate from the BMD dataset. Because of the complex network structure used, the data from ECG-ID does not produce substantial results.

## Verification

The SNN was trained on 100 epochs with Model Checkpoint and early stopping in place tracking validation loss. Together with the Euclidean Distance, the SNN uses contrastive loss, which takes the output of the network for a positive example and calculates its distance to an example of the same class and contrasts that with the distance to negative examples.

On average, the training period lasts for a 20 – 25 minutes. The SNN model achieved average results, Figure 17 and Figure 18, whereby the validation loss is 49.69%. After numerous experiments and observations, the decision threshold margin of enrolled against unenrolled test sample is 0.00099999 meaning if the similarity score is above or equal to 0.00099999, then such egg segment resembles one of the enrolled templates hence a successful verification. Test samples are illustrated in Figure 19.

Chart

Description automatically generated with medium confidence

Figure 17 Training and Validation loss for the SNN model

Chart, line chart

Description automatically generated

Figure 18 Training results for the SNN. In Blue is the Training loss and Red is Validation Loss

Calendar

Description automatically generated with low confidence

Figure 19 Predicted test samples from the SNN model

## Authentication.

On average, the training period lasts for 1 hour. The CNN model was successfully trained on 100 epochs with early stopping, Model Checkpoint on Validation loss and optimally completed on after an average of 20-25 epochs. The results for the model are substantially excellent given the short duration and complex network structure. The CNN model achieved an accuracy score of 99.93% and validation loss of 0.32% is displayed in Figure 19 and Figure 20. The CNN model has a threshold margin of 99%, meaning for the test data selected of size 47729, 47459 segments are correctly classified with an accuracy of >= 99%, and 270 segments have an accuracy score <= 99%.

Chart

Description automatically generated

Figure 20 Training and Validation Accuracy scores

Chart

Description automatically generated

Figure 21 Training and Validation Loss scores

The confusion matrix is displayed in Figure 21, which corresponds to the precision, recall and f1-score all at 100%. Figure 22 displays several predicted samples.

Chart, scatter chart

Description automatically generated

Figure 22 Confusion Matrix of the CNN model

A picture containing text

Description automatically generated

Figure 23 Predicted test samples from the CNN model

# DISCUSSION

The performed approach aims to employ Deep Learning as a robust candidate for an ECG Biometric System. The goal is to design an effective enrolment, verification, and authentication strategies for continuous authentication systems. There's an increase in the development of Deep Learning ECG-Based Biometrics [13] [14] [38] [16], which shows promising results. However, most studies only focused on closed-set classification. Though Debbis achieved average results with the Siamese Neural Network model, the implementation of the authentication using the Convolutional Neural Network provides another layer of security to the system.

Despite significant research progress, the ECG-ID dataset in use contains a low number of classes to produce a robust and industry dependable Deep Learning model hence only the MIT-BIH and the BMD dataset were utilized. Also, few industry-level datasets dedicated to user identification and authentication exist [11], and a large section of them are not publicly available or may require special access based on research merit. Subjectively on progress, the study development could be faster to enable enough time for testing and evaluation. Areas I could improve is sufficient time allocation for the project.

# ETHICS and PROFESSIONAL CONDUCT

The major ethical implications in the field of Biometrics, particularly ECGs, are privacy and confidentiality. If privacy implies having power over how and when we are portrayed to others, then biometrics that identifies us uniquely may easily violate our fundamental privacy. This is particularly true when you realise that users do not monitor the selection, storage, or use of these identities. One of the main benefits of a biometric signature is that it is unique to each person and does not change over time. Ironically, invariability is perhaps one of the vulnerabilities of biometric systems. Your identity and security are compromised forever if the system is breached. We can't change our physical features, like changing a password.

# CONCLUSIONS

The report presents the Debbis, an ECG-based biometric approach based on deep learning. Through the use of Siamese and Convolutional Neural Networks to extract features that allow performing a closed-set identification, identity verification and periodic re-authentication. To evaluate the performance of the study, the model will be tested on test samples obtained from the ECG-ID database for closed-set identification, identity verification and authentication. Future work beyond this study should regard the development of comprehensive ECG datasets to allow advanced exploration into secure biometric systems. Despite both fields being under development and novice, biometric systems will significantly benefit from neural network incremental learning.

# REFERENCES

|  |  |
| --- | --- |
| [1] | A. Nait-Ali, “Hidden biometrics: Towards using biosignals and biomedical images for security applications,” *International Workshop on Systems, Signal Processing and their Applications, WOSSPA,* pp. 352-356, 2011. |
| [2] | J. D. Woodward, N. M. Orlans and P. T. Higgins, Biometrics, New York: McGraw-Hill/Osborne, 2003. |
| [3] | V. K. Raina, “Emerging Technologies for User-Friendly Mobile Payment Applications,” *Electronic Payment Systems for Competitive Advantage in E-Commerce,* pp. 279-307, 2014. |
| [4] | A. M. Abhishek and H. N. Suma, “Comparison of biosignal Electrocardiography (ECG), Fingerprint and Iris as Biometrics authentication tool,” *2014 IEEE Conference on Biomedical Engineering and Sciences (IECBES),* pp. 303-308, 2014. |
| [5] | J. Feher, “The Cardiac Action Potential,” in *Quantitative Human Physiology*, Amsterdam, Elsevier, 2012, pp. 528-536. |
| [6] | Y. N. Singh and P. Gupta, “ECG to Individual Identification,” *2008 IEEE Second International Conference on Biometrics: Theory, Applications and Systems ,* pp. 1-8, 2008. |
| [7] | F. Agrafioti and D. Hatzinakos, “ECG biometric analysis in cardiac irregularity conditions,” *Signal, Image and Video Processing,* vol. 3, no. 4, p. 329, 2009. |
| [8] | M. N. Dar, M. U. Akram, A. Shaukat and M. A. Khan, “ECG Based Biometric Identification for Population with Normal and Cardiac Anomalies Using Hybrid HRV and DWT Features,” *2015 5th International Conference on IT Convergence and Security (ICITCS),* pp. 1-5, 2015. |
| [9] | S. Raschka, J. Patterson and C. Nolet, “Machine Learning in Python: Main Developments and Technology Trends in Data Science, Machine Learning, and Artificial Intelligence,” *Information,* vol. 11, no. 4, p. 193, 2020. |
| [10] | I. Odinaka, P.-H. Lai, A. D. Kaplan, J. A. O'Sullivan, E. J. Sirevaag and J. W. Rohrbaugh, “ECG Biometric Recognition: A Comparative Analysis,” *IEEE Transactions on Information Forensics and Security,* vol. 7, no. 6, pp. 1812-1824, 2012. |
| [11] | M. Merone, P. Soda, M. Sansone and C. Sansone, “ECG databases for biometric systems: A systematic review,” *Expert Systems with Applications,* vol. 67, pp. 189-202, 2017. |
| [12] | D. P. Coutinho, H. Silva, H. Gamboa, A. Fred and M. Figueiredo, “Novel fiducial and non-fiducial approaches to electrocardiogram-based biometric systems,” *IET Biometrics,* vol. 2, no. 2, pp. 64-75, 2013. |
| [13] | A. Eduardo, H. Aidos and A. Fred, “ECG-based biometrics using a deep autoencoder for feature learning-an empirical study on transferability.,” *International Conference on Pattern Recognition Applications and Methods,* vol. 2, pp. 463-470, 2017. |
| [14] | Q. Zhang, D. Zhou and X. Zeng, “PulsePrint: Single-arm-ECG biometric human identification using deep learning,” *2017 IEEE 8th Annual Ubiquitous Computing, Electronics and Mobile Communication Conference (UEMCON),* pp. 452-456, 2017. |
| [15] | R. D. Labati, R. Sassi and F. Scotti, “ECG biometric recognition: Permanence analysis of QRS signals for 24 hours continuous authentication,” *2013 IEEE international workshop on information forensics and security (WIFS),* pp. 31-36, 2013. |
| [16] | D. Belo, N. Bento, H. Silva, A. Fred and H. Gamboa, “ECG Biometrics Using Deep Learning and Relative Score Threshold Classification,” *Sensors,* vol. 20, no. 15, p. 4078, 2020. |
| [17] | C. Geng, S.-j. Huang and S. Chen, “ Recent advances in open set recognition: A survey.,” *IEEE transactions on pattern analysis and machine intelligence,* 2020. |
| [18] | J. R. Pinto, J. S. Cardoso and A. Lourenço, “Pinto, J. R., Cardoso, J. S., & Lourenço, A. (2018). Evolution, current challenges, and future possibilities in ECG biometrics.,” *IEEE Access,* vol. 6, pp. 34746-34776, 2018. |
| [19] | W. Scheirer, A. Rocha, A. Sapkota and T. Boult, “Toward Open Set Recognition,” *IEEE transactions on pattern analysis and machine intelligence,* 2013. |
| [20] | L. Fei-Fei, R. Fergus and P. Perona, “One-shot learning of object categories,” *IEEE transactions on pattern analysis and machine intelligence,* vol. 28, no. 4, pp. 594-611, 2006. |
| [21] | B. M. Lake, R. Salakhutdinov and J. B. Tenenbaum, “One-shot learning by inverting a compositional causal process,” *Advances in Neural Information Processing Systems 26 (NIPS 2013),* 2013. |
| [22] | L. Fe-Fei, “ A Bayesian approach to unsupervised one-shot learning of object categories.,” *Proceedings Ninth IEEE International Conference on Computer Vision,* pp. 1134-1141, 2003. |
| [23] | J. Snell, K. Swersky and R. S. Zemel, “Prototypical networks for few-shot learning,” *arXiv preprint,* 2017. |
| [24] | Z. Chen, Y. Fu, Y. Zhang, Y. G. Jiang, X. Xue and L. Sigal, “Semantic feature augmentation in few-shot learning,” *arXiv preprint,* pp. 86-89, 2018. |
| [25] | K. Simonyan and A. Zisserman, “Very deep convolutional networks for large-scale image recognition,” *arXiv preprint arXiv:1409.1556,* 2014. |
| [26] | C. Szegedy, V. Vanhoucke, S. Ioffe, J. Shlens and Z. Wojna, “Rethinking the Inception Architecture for Computer Vision,” *Proceedings of the IEEE conference on computer vision and pattern recognition,* pp. 2818-2826, 2016. |
| [27] | D. D. Chakladar, P. Kumar, P. P. Roy, D. P. Dogra, E. Scheme and V. Chang, “A multimodal-Siamese Neural Network (mSNN) for person verification using signatures and EEG,” *nformation Fusion,* vol. 71, pp. 17-27, 2021. |
| [28] | E. Maiorana, “ EEG-based biometric verification using Siamese CNNs,” *International Conference on Image Analysis and Processing,* pp. 3-11, 2019. |
| [29] | V. Singh, S. Tewary, V. Sardana and H. K. Sardana, “Singh, V., Tewary, S., Sardana, V., & Sardana, H. K. (2019, March). Arrhythmia Detection-A Machine Learning based Comparative Analysis with MIT-BIH ECG Data.,” *IEEE 5th International Conference for Convergence in Technology,* pp. 1-15, 2019. |
| [30] | A. L. Goldberger, L. A. N. Amaral, L. Glass, J. M. Hausdorff, P. C. Ivanov, R. G. Mark, J. E. Mietus, G. B. Moody, C.-K. Peng and H. E. Stanley, “PhysioBank, PhysioToolkit, and PhysioNet: components of a new research resource for complex physiologic signals.,” *Circulation,* vol. 101, no. 23, pp. e215-e220, 2000. |
| [31] | T. S. Lugovaya, “Biometric human identification based on electrocardiogram,” *Master's thesis, Faculty of Computing Technologies and Informatics, Electrotechnical University ‘LETI’, Saint-Petersburg, Russian Federation,* 2005. |
| [32] | E. Ihsanto, K. Ramli, D. Sudiana and S. T. Gunawan, “Fast and accurate algorithm for ECG authentication using residual depthwise separable convolutional neural networks.,” *Applied Sciences,* vol. 10, no. 9, p. 3304, 2020. |
| [33] | R. Salloum and C.-C. J. Kuo, “Ecg-based biometrics using recurrent neural networks.,” *2017 IEEE International Conference on Acoustics, Speech and Signal Processing (ICASSP),* pp. 2062-2066, 2017. |
| [34] | G. B. Moody, “Installing the WFDB Software Package,” PhysioNet, [Online]. Available: https://www.physionet.org/physiotools/wag/install.htm. [Accessed December 2020]. |
| [35] | I. I. Christov, “Real time electrocardiogram QRS detection using combined adaptive threshold,” *Biomedical engineering online,* vol. 3, no. 1, pp. 1-9, 2004. |
| [36] | P. Hamilton, “Open source ECG analysis,” *Computers in cardiology,* pp. 101-104, 2002. |
| [37] | F. Canento, A. Lourenc, H. Silva and A. Fred, “Review and Comparison of Real Time Electrocardiogram Segmentation Algorithms for Biometric Applications,” *Proc. 6th Int. Conf. Health Inform,* 2013. |
| [38] | R. D. Labati, E. Muñoz, V. Piuri, R. Sassi and F. Scotti, “Deep-ECG: Convolutional Neural Networks for ECG biometric recognition,” *Pattern Recognition Letters,* vol. 126, pp. 78-85, 2019. |
| [39] | Y. Wu, F. Yang, Y. Liu, X. Zha and S. Yuan, “A Comparison of 1-D and 2-D Deep Convolutional Neural Networks in ECG Classification,” *arXiv preprint arXiv:1810.07088,* 2018. |
| [40] | G. B. Moody and R. G. Mark, “The impact of the MIT-BIH arrhythmia database,” *Moody, G. B., & Mark, R. G. (2001). The impact of the MIT-BIH arrhythmia database. IEEE Engineering in Medicine and Biology Magazine,* vol. 20, no. 3, pp. 45-50, 2001. |
| [41] | J. R. Pinto, J. S. Cardoso and A. Lourenço, “Deep neural networks for biometric identification based on non-intrusive ECG acquisitions.,” *The Biometric Computing,* pp. 217-234, 2019. |
| [42] | G. B. A. Salomon, R. H. Vareto, W. R. Schwartz and D. Menotti, “Open-set Face Recognition for Small Galleries Using Siamese Networks,” *2020 International Conference on Systems, Signals and Image Processing (IWSSIP),* pp. 161-166, 2020. |
| [43] | G. Koch, R. Zemel and R. Salakhutdinov, “Siamese Neural Networks for One-shot Image Recognition,” *ICML deep learning workshop,* vol. 2, 2015. |